hd44780_I2Clcd examples
=======================

The examples included in this directory are for the hd44780_I2Clcd i/o class.<br>
The hd44780_I2Clcd i/o class controls an LCD with a native i2c interface that uses chips like the PCF2116, PCF2119x etc...

#### The following examples are included:

- `HelloWorld`<br>
Prints "Hello, World!" on the lcd

- `LCDCustomChars`<br>
Demonstrates using custom characters

- `LineWrap`<br>
Demonstrates automatic linewrap functionality

- `Serial2LCD`<br>
Displays a message read from the serial port on the lcd.

- `UpTime`<br>
Prints the amount of time since the Arduino has been reset.

- `hd44780examples`<br>
The hd44780examples subdirectory contains
hd44780_I2Clcd class specific wrapper sketches for sketches under
examples/hd44780examples.
